	*** PVs_PSI-0.1_LN-CutOff-120_LN-HWHM-1.05_PE-beta-1000_PE-CutOff-10_PE-HWHM-8.65_Length-100 *** 

	---------- OUT-parameters ----------
	Vector Length [s]           	 100
	Sample Rate [1/s]           	 10000
	Mean Vector-Power [W]       	 1.002
	PSI of combined vector [1]  	 0.10
	beta of PE vector [1]       	 977.40
	HWHM Combined vector [ms]   	 1.05
	HWHM Atmosphere only [ms]   	 1.05
	LowPass Atmosphere only [Hz]  	 120.00
	HWHM Pointing only [ms]     	 8.65
	LowPass Pointing only [Hz]  	 10.00

