	*** PVs_PSI-0.1_LN-CutOff-40_LN-HWHM-3.15_PE-beta-1000_PE-CutOff-10_PE-HWHM-8.75_Length-100 *** 

	---------- OUT-parameters ----------
	Vector Length [s]           	 100
	Sample Rate [1/s]           	 10000
	Mean Vector-Power [W]       	 0.999
	PSI of combined vector [1]  	 0.10
	beta of PE vector [1]       	 961.83
	HWHM Combined vector [ms]   	 3.15
	HWHM Atmosphere only [ms]   	 3.15
	LowPass Atmosphere only [Hz]  	 40.00
	HWHM Pointing only [ms]     	 8.75
	LowPass Pointing only [Hz]  	 10.00

