*** PVs_PSI-0.4_LN-CutOff-120_LN-HWHM-0.95_PE-beta-1000_PE-CutOff-10_PE-HWHM-8.55_Length-100 *** 

---------- OUT-parameters ----------
Vector Length [s]           	 100
Sample Rate [1/s]           	 10000
Mean Vector-Power [W]       	 1.001
PSI of combined vector [1]  	 0.40
beta of PE vector [1]       	 1021.04
HWHM Combined vector [ms]   	 0.95
HWHM Atmosphere only [ms]   	 0.95
LowPass Atmosphere only [Hz]  	 120.00
HWHM Pointing only [ms]     	 8.55
LowPass Pointing only [Hz]  	 10.00

